IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "Option [Entire project;Keep GUIDs;All Domain;All elements;All struct.;scale:100.000000;CSG:Extruded;Comp. wall:Extruded;Building element parts;Chained beam:Extruded;Comp. slab:Extruded]"
File name: "E:\lab\æ¯è®¾å·¥ä½\å®éªæ¨¡å\è®ºæä¸­å®éªçæ¨¡å\æ¶é´ç©ºé´\M4-b(å«å¢ 4)Archicad.ifc"
Time stamp: "2015-05-02T21:58:18"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "PreProc - EDM 5.0"
Originating system: "IFC file generated by Graphisoft ArchiCAD-64 16.0.0 CHI FULL Windows version (IFC2x3 add-on version: 3270 CHI FULL)."
Authorization: "The authorising person"
Application: "ArchiCAD-64" version "16.0.0" identifier "IFC2x3 add-on version: 3270 CHI FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Î´¶¨Òå" of Organization "Î´¶¨Òå"
  Owner history of Person "Î´¶¨Òå" of Organization "Î´¶¨Òå" | application "ArchiCAD-64" version "16.0.0" identifier "IFC2x3 add-on version: 3270 CHI FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change ADDED | created 1430575097 (2015-05-02T13:58:17Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Default Project"
  IFCSITE "Default Site" | latitude 35° 42′ 0″ | longitude 139° 46′ 0″
    IFCBUILDING "M4-b(±ðÊû4)" | postal address (none given)
      IFCBUILDINGSTOREY "GL" | elevation 0.
      IFCBUILDINGSTOREY "1F" | elevation 300.
        contains 49 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "ëÌ|ALC 100" | names: "W013" | material: layers "ëÌ|ALC 100" ("ëÌ|ALC" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOH96A3A001H4782f7fe1" | names: "001" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "W-RC 20+160 180" | names: "W012", "W009", "W011" (+1 more) | material: layers "W-RC 20+160" ("ëÌ|RCitJVj" 20., "ëÌ|RC" 160.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH383D1A5FH4782f7fe3" | names: "002" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIHB652A559H4782f7fe2" | names: "001" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH32BF7FB2H4782f7ff5" | names: "001" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOHCD46EB90H4782f7fe4" | names: "004" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "ëÌ|RC 180" | names: "W023", "W024", "W025" (+1 more) | material: layers "ëÌ|RC 180" ("ëÌ|RC" 180.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH78CC732FH4782f7ff6" | names: "008" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH10723F62H4782f7ff7" | names: "006" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH8F61781DH4782f7ff8" | names: "007" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH7BBF3D86H4782f7ffa" | names: "002" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOHDFC56289H4782f7ff9" | names: "001" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "ëÌ|CB(ÓÙÀÙ[U) 100" | names: "W027" | material: layers "ëÌ|CB(ÓÙÀÙ[U) 100" ("ëÌ|CB(ÓÙÀÙ[U)" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOHDFC56289H4782f7ff9" | names: "008" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOH72A48315H4782f7ffb" | names: "007" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCSTAIR | STRAIGHT_RUN_STAIR | names: "Ki-001" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "D500" | object type "D500" | names: "C010", "C011" | material: "ëÌ|RC" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "500X500" | object type "500X500" | names: "C001", "C002", "C005" (+3 more) | material: "ëÌ|RC" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "IFC½ØÃæ" | object type "IFC½ØÃæ" | names: "C015", "C014", "C017" (+2 more) | material: "ëÌ|RC" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          5 x IFCBEAM | type IFCBEAMTYPE "500X400" | object type "500X400" | names: "B005", "B006", "B007" (+2 more) | material: "ëÌ|RC" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          8 x IFCSLAB | FLOOR | names: "S005", "S010", "S013" (+3 more) | material: layers "ëÌ|RC 200" ("ëÌ|RC" 200.); layers "ëÌ|RC 150" ("ëÌ|RC" 150.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
        IFCSPACE "07" | long name "Lobby" | INTERNAL
        IFCSPACE "08" | long name "Meeting room" | INTERNAL
        IFCSPACE "10" | long name "Washroom" | INTERNAL
        IFCSPACE "11" | long name "Washroom" | INTERNAL
        IFCSPACE "09" | long name "Meeting space" | INTERNAL
      IFCBUILDINGSTOREY "2F" | elevation 3700.
        contains 38 elements
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "W-RC 20+160 180" | names: "W014", "W016", "W015" (+7 more) | material: layers "W-RC 20+160" ("ëÌ|RCitJVj" 20., "ëÌ|RC" 160.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "ëÌ|ALC 100" | names: "W013", "W020" | material: layers "ëÌ|ALC 100" ("ëÌ|ALC" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOH3763C3A6H4782f801d" | names: "001" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH32BF7FB2H4782f7ff5" | names: "001" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2XDOH63C531B1H4782f801e" | names: "006" | material: "±³¾°" | property sets: Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH6AB7CF0BH4782f801f" | names: "005" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIH6AB7CF0BH4782f801f" | names: "004" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIHB652A559H4782f7fe2" | names: "001" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "IFC2XWIHB652A559H4782f7fe2" | names: "001" | material: "±³¾°" | property sets: Pset_WindowCommon_Jpn, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2x_SnglDoorSnglSwing" | names: "003" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "IFC2x_SnglDoorSnglSwing" | names: "002" | material: "±³¾°" | property sets: Pset_DoorCommon_Jpn, Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing
          2 x IFCRAILING | HANDRAIL | names: "001", "002" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "500X500" | object type "500X500" | names: "C002", "C005", "C004" (+3 more) | material: "ëÌ|RC" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          5 x IFCBEAM | type IFCBEAMTYPE "500X400" | object type "500X400" | names: "B005", "B006", "B007" (+2 more) | material: "ëÌ|RC" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          4 x IFCSLAB | FLOOR | names: "S003", "S001", "S012" | material: layers "ëÌ|RC 200" ("ëÌ|RC" 200.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
        IFCSPACE "06" | long name "Office" | INTERNAL
        IFCSPACE "04" | long name "Common space" | INTERNAL
        IFCSPACE "14" | long name "Lounge" | INTERNAL
        IFCSPACE "05" | long name "Office" | INTERNAL
      IFCBUILDINGSTOREY "RF" | elevation 7100.
        contains 3 elements
          2 x IFCSLAB | FLOOR | names: "S001", "S003" | material: layers "ëÌ|RC 200" ("ëÌ|RC" 200.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | ROOF | names: "S011" | material: "±³¾°" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing

Types
  IFCWALLTYPE "ëÌ|ALC 100" | 3 occurrences
  IFCDOORSTYLE "IFC2XDOH96A3A001H4782f7fe1" | 1 occurrence
  IFCWALLTYPE "W-RC 20+160 180" | 14 occurrences
  IFCWINDOWSTYLE "IFC2XWIH383D1A5FH4782f7fe3" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIHB652A559H4782f7fe2" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH32BF7FB2H4782f7ff5" | 1 occurrence
  IFCDOORSTYLE "IFC2XDOHCD46EB90H4782f7fe4" | 1 occurrence
  IFCWALLTYPE "ëÌ|RC 180" | 4 occurrences
  IFCWINDOWSTYLE "IFC2XWIH78CC732FH4782f7ff6" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH10723F62H4782f7ff7" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH8F61781DH4782f7ff8" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH7BBF3D86H4782f7ffa" | 1 occurrence
  IFCDOORSTYLE "IFC2XDOHDFC56289H4782f7ff9" | 1 occurrence
  IFCWALLTYPE "ëÌ|CB(ÓÙÀÙ[U) 100" | 1 occurrence
  IFCDOORSTYLE "IFC2XDOHDFC56289H4782f7ff9" | 1 occurrence
  IFCDOORSTYLE "IFC2XDOH72A48315H4782f7ffb" | 1 occurrence
  IFCCOLUMNTYPE "D500" | 2 occurrences
  IFCCOLUMNTYPE "500X500" | 12 occurrences
  IFCCOLUMNTYPE "IFC½ØÃæ" | 5 occurrences
  IFCBEAMTYPE "500X400" | 10 occurrences
  IFCDOORSTYLE "IFC2XDOH3763C3A6H4782f801d" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH32BF7FB2H4782f7ff5" | 1 occurrence
  IFCDOORSTYLE "IFC2XDOH63C531B1H4782f801e" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH6AB7CF0BH4782f801f" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIH6AB7CF0BH4782f801f" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIHB652A559H4782f7fe2" | 1 occurrence
  IFCWINDOWSTYLE "IFC2XWIHB652A559H4782f7fe2" | 1 occurrence
  IFCDOORSTYLE "IFC2x_SnglDoorSnglSwing" | SINGLE_SWING_LEFT | 1 occurrence
  IFCDOORSTYLE "IFC2x_SnglDoorSnglSwing" | SINGLE_SWING_RIGHT | 1 occurrence

Property sets
  AC_Pset_Name | properties | on 9 objects (5 IFCWINDOW, 3 IFCDOOR, 1 IFCRAILING)
    Name = "001" (IFCLABEL)
  AC_Pset_Name | properties | on 4 objects (2 IFCWINDOW, 1 IFCDOOR, 1 IFCRAILING)
    Name = "002" (IFCLABEL)
  AC_Pset_Name | properties | on 3 objects (3 IFCSLAB)
    Name = "S001" (IFCLABEL)
  AC_Pset_Name | properties | on 3 objects (3 IFCSLAB)
    Name = "S003" (IFCLABEL)
  AC_Pset_Name | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Name = "W013" (IFCLABEL)
  AC_Pset_Name | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Name = "W012" (IFCLABEL)
  AC_Pset_Name | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Name = "W009" (IFCLABEL)
  AC_Pset_Name | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Name = "004" (IFCLABEL)
  AC_Pset_Name: 53 more contents on 72 objects not shown
  AC_Pset_RenovationAndPhasing | properties | on 99 objects (22 IFCWALLSTANDARDCASE, 19 IFCCOLUMN, 15 IFCSLAB, 12 IFCWINDOW)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALLSTANDARDCASE)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_DoorCommon_Jpn | properties | on 3 objects (3 IFCDOOR)
    airproof = "¢è" (IFCLABEL)
    chainlock = "¢è" (IFCLABEL)
    chiri_inside = 11. (IFCREAL)
    chiri_outside = 10. (IFCREAL)
    closing_priority = "¢è" (IFCLABEL)
    cylinder_side = "¢è" (IFCLABEL)
    door_bumper = "¢è" (IFCLABEL)
    door_closer = "¢è" (IFCLABEL)
    door_stopper = "¢è" (IFCLABEL)
    fixture_handle = "¢è" (IFCLABEL)
    fixture_support = "¢è" (IFCLABEL)
    floor_level_difference = 100. (IFCREAL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 201. (IFCREAL)
    frame_width = 25. (IFCREAL)
    glass_type = "¢è" (IFCLABEL)
    height = 2100. (IFCREAL)
    in_out = "à" (IFCLABEL)
    louver_finish = "¢è" (IFCLABEL)
    louver_material = "¢è" (IFCLABEL)
    louver_mechanism = "¢è" (IFCLABEL)
    louver_shape = "¢è" (IFCLABEL)
    name_of_maker = "" (IFCLABEL)
    opening_bottom_distance = 150. (IFCREAL)
    opening_distance = 150. (IFCREAL)
    opening_height_bottom = 500. (IFCREAL)
    opening_height_top = 800. (IFCREAL)
    opening_top_distance = 150. (IFCREAL)
    opening_width = 150. (IFCREAL)
    others = "" (IFCLABEL)
    panel_finish = "¢è" (IFCLABEL)
    panel_material = "¢è" (IFCLABEL)
    panel_style = "tbV" (IFCLABEL)
    panel_thickness = 45. (IFCREAL)
    panel_type = "¢è" (IFCLABEL)
    peephole = "¢è" (IFCLABEL)
    postbox = "¢è" (IFCLABEL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "ÐJ«Ë" (IFCLABEL)
    side_frame_shape = 1 (IFCINTEGER)
    side_frame_width = 25. (IFCREAL)
    soundproof = "¢è" (IFCLABEL)
    threshold_material = "¢è" (IFCLABEL)
    threshold_shape = 6 (IFCINTEGER)
    top_frame_shape = 1 (IFCINTEGER)
    transom_height = 0. (IFCREAL)
    transom_style = "Â" (IFCLABEL)
    type_name = "SD" (IFCLABEL)
    type_no = 10 (IFCINTEGER)
    width = 900. (IFCREAL)
  Pset_DoorCommon_Jpn | properties | on 1 object (1 IFCDOOR)
    airproof = "¢è" (IFCLABEL)
    chainlock = "¢è" (IFCLABEL)
    chiri_inside = 10. (IFCREAL)
    chiri_outside = 10. (IFCREAL)
    closing_priority = "¢è" (IFCLABEL)
    cylinder_side = "¢è" (IFCLABEL)
    door_bumper = "¢è" (IFCLABEL)
    door_closer = "¢è" (IFCLABEL)
    door_stopper = "¢è" (IFCLABEL)
    fixture_handle = "¢è" (IFCLABEL)
    fixture_support = "¢è" (IFCLABEL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 120. (IFCREAL)
    frame_width = 25. (IFCREAL)
    glass_type = "¢è" (IFCLABEL)
    height = 2100. (IFCREAL)
    in_out = "à" (IFCLABEL)
    louver_finish = "¢è" (IFCLABEL)
    louver_material = "¢è" (IFCLABEL)
    louver_mechanism = "¢è" (IFCLABEL)
    louver_shape = "¢è" (IFCLABEL)
    name_of_maker = "" (IFCLABEL)
    opening_bottom_distance = 150. (IFCREAL)
    opening_distance = 150. (IFCREAL)
    opening_height_bottom = 500. (IFCREAL)
    opening_height_top = 800. (IFCREAL)
    opening_top_distance = 150. (IFCREAL)
    opening_width = 150. (IFCREAL)
    others = "" (IFCLABEL)
    panel_finish = "¢è" (IFCLABEL)
    panel_material = "¢è" (IFCLABEL)
    panel_style = "tbV" (IFCLABEL)
    panel_thickness = 45. (IFCREAL)
    panel_type = "¢è" (IFCLABEL)
    peephole = "¢è" (IFCLABEL)
    postbox = "¢è" (IFCLABEL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "©RJ«Ë" (IFCLABEL)
    side_frame_shape = 3 (IFCINTEGER)
    side_frame_width = 25. (IFCREAL)
    soundproof = "¢è" (IFCLABEL)
    threshold_material = "¢è" (IFCLABEL)
    threshold_shape = 1 (IFCINTEGER)
    top_frame_shape = 3 (IFCINTEGER)
    transom_height = 0. (IFCREAL)
    transom_style = "Â" (IFCLABEL)
    type_name = "SD" (IFCLABEL)
    type_no = 6 (IFCINTEGER)
    width = 1500. (IFCREAL)
  Pset_DoorCommon_Jpn | properties | on 1 object (1 IFCDOOR)
    airproof = "¢è" (IFCLABEL)
    chainlock = "¢è" (IFCLABEL)
    chiri_inside = 10. (IFCREAL)
    chiri_outside = 10. (IFCREAL)
    closing_priority = "¢è" (IFCLABEL)
    cylinder_side = "¢è" (IFCLABEL)
    door_bumper = "¢è" (IFCLABEL)
    door_closer = "¢è" (IFCLABEL)
    door_stopper = "¢è" (IFCLABEL)
    fixture_handle = "¢è" (IFCLABEL)
    fixture_support = "¢è" (IFCLABEL)
    floor_level_difference = 100. (IFCREAL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 120. (IFCREAL)
    frame_width = 25. (IFCREAL)
    glass_type = "¢è" (IFCLABEL)
    height = 2100. (IFCREAL)
    in_out = "à" (IFCLABEL)
    louver_finish = "¢è" (IFCLABEL)
    louver_material = "¢è" (IFCLABEL)
    louver_mechanism = "¢è" (IFCLABEL)
    louver_shape = "¢è" (IFCLABEL)
    main_panel_width = 900. (IFCREAL)
    name_of_maker = "" (IFCLABEL)
    opening_bottom_distance = 150. (IFCREAL)
    opening_distance = 150. (IFCREAL)
    opening_height_bottom = 500. (IFCREAL)
    opening_height_top = 800. (IFCREAL)
    opening_top_distance = 150. (IFCREAL)
    opening_width = 150. (IFCREAL)
    others = "" (IFCLABEL)
    panel_finish = "¢è" (IFCLABEL)
    panel_material = "¢è" (IFCLABEL)
    panel_style = "tbV" (IFCLABEL)
    panel_thickness = 45. (IFCREAL)
    panel_type = "¢è" (IFCLABEL)
    peephole = "¢è" (IFCLABEL)
    postbox = "¢è" (IFCLABEL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "eqJ«Ë" (IFCLABEL)
    side_frame_shape = 1 (IFCINTEGER)
    side_frame_width = 25. (IFCREAL)
    side_opening_bottom_distance = 150. (IFCREAL)
    side_opening_distance = 150. (IFCREAL)
    side_opening_height_bottom = 500. (IFCREAL)
    side_opening_height_top = 800. (IFCREAL)
    side_opening_top_distance = 150. (IFCREAL)
    side_panel_style = "tbV" (IFCLABEL)
    side_panel_width = 900. (IFCREAL)
    soundproof = "¢è" (IFCLABEL)
    threshold_material = "¢è" (IFCLABEL)
    threshold_shape = 1 (IFCINTEGER)
    top_frame_shape = 1 (IFCINTEGER)
    transom_height = 0. (IFCREAL)
    transom_style = "KXÍßEµ" (IFCLABEL)
    type_name = "SD" (IFCLABEL)
    type_no = 7 (IFCINTEGER)
    width = 1350. (IFCREAL)
  Pset_DoorCommon_Jpn | properties | on 1 object (1 IFCDOOR)
    Name = "003" (IFCLABEL)
    frame_material = "14" (IFCLABEL)
    frame_thicknrss = 0.1 (IFCREAL)
    frame_width = 0.05 (IFCREAL)
    height = 2.1 (IFCREAL)
    width = 1. (IFCREAL)
  Pset_DoorCommon_Jpn | properties | on 1 object (1 IFCDOOR)
    Name = "002" (IFCLABEL)
    frame_material = "14" (IFCLABEL)
    frame_thicknrss = 0.1 (IFCREAL)
    frame_width = 0.05 (IFCREAL)
    height = 2.1 (IFCREAL)
    width = 1. (IFCREAL)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "SD-10" (IFCLABEL)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExterior = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IFC2X_SINGLE" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireExit = FALSE (IFCBOOLEAN)
    IsExterior = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "SD-6" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SD-10" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExterior = FALSE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "SD-11" (IFCLABEL)
  Pset_WindowCommon_Jpn | properties | on 5 objects (5 IFCWINDOW)
    airproof = "¢è" (IFCLABEL)
    board_finish = "¢è" (IFCLABEL)
    board_material = "¢è" (IFCLABEL)
    board_thickness = 50. (IFCREAL)
    board_width = 25. (IFCREAL)
    chiri_inside = 0.01 (IFCREAL)
    chiri_outside = 0.015 (IFCREAL)
    extra_metalwork = "¢è" (IFCLABEL)
    frame_board_distance = 15. (IFCREAL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 70. (IFCREAL)
    frame_width = 15. (IFCREAL)
    glass_fixing = "¢è" (IFCLABEL)
    glass_type = "¢è" (IFCLABEL)
    height = 1200. (IFCREAL)
    in_out = "O" (IFCLABEL)
    jamb_depth = 60. (IFCREAL)
    jamb_shape = "1" (IFCLABEL)
    jamb_width_side = 60. (IFCREAL)
    jamb_width_top = 60. (IFCREAL)
    manual_opener = "¢è" (IFCLABEL)
    name_of_maker = "" (IFCLABEL)
    net_shape = "¢è" (IFCLABEL)
    net_type = "¢è" (IFCLABEL)
    others = "" (IFCLABEL)
    outside_board_width = 25. (IFCREAL)
    overhang = 85. (IFCREAL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "ø«á¢" (IFCLABEL)
    sill_finish = "¢è" (IFCLABEL)
    sill_material = "¢è" (IFCLABEL)
    soundproof = "¢è" (IFCLABEL)
    type_name = "AW" (IFCLABEL)
    type_no = 1 (IFCINTEGER)
    waterproof = "¢è" (IFCLABEL)
    width = 1600. (IFCREAL)
  Pset_WindowCommon_Jpn | properties | on 2 objects (2 IFCWINDOW)
    airproof = "¢è" (IFCLABEL)
    board_finish = "¢è" (IFCLABEL)
    board_material = "¢è" (IFCLABEL)
    board_thickness = 50. (IFCREAL)
    board_width = 25. (IFCREAL)
    chiri_inside = 0.01 (IFCREAL)
    chiri_outside = 0.015 (IFCREAL)
    extra_metalwork = "¢è" (IFCLABEL)
    frame_board_distance = 15. (IFCREAL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 70. (IFCREAL)
    frame_width = 15. (IFCREAL)
    glass_fixing = "¢è" (IFCLABEL)
    glass_type = "¢è" (IFCLABEL)
    height = 1800. (IFCREAL)
    in_out = "O" (IFCLABEL)
    jamb_depth = 60. (IFCREAL)
    jamb_shape = "1" (IFCLABEL)
    jamb_width_side = 60. (IFCREAL)
    jamb_width_top = 60. (IFCREAL)
    manual_opener = "¢è" (IFCLABEL)
    name_of_maker = "" (IFCLABEL)
    net_shape = "¢è" (IFCLABEL)
    net_type = "¢è" (IFCLABEL)
    others = "" (IFCLABEL)
    outside_board_width = 25. (IFCREAL)
    overhang = 85. (IFCREAL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "ø«á¢" (IFCLABEL)
    sill_finish = "¢è" (IFCLABEL)
    sill_material = "¢è" (IFCLABEL)
    soundproof = "¢è" (IFCLABEL)
    type_name = "AW" (IFCLABEL)
    type_no = 3 (IFCINTEGER)
    waterproof = "¢è" (IFCLABEL)
    width = 1600. (IFCREAL)
  Pset_WindowCommon_Jpn | properties | on 1 object (1 IFCWINDOW)
    airproof = "¢è" (IFCLABEL)
    board_finish = "¢è" (IFCLABEL)
    board_material = "¢è" (IFCLABEL)
    board_thickness = 111. (IFCREAL)
    board_width = 25. (IFCREAL)
    chiri_inside = 0.041 (IFCREAL)
    chiri_outside = 0.01 (IFCREAL)
    extra_metalwork = "¢è" (IFCLABEL)
    frame_board_distance = 15. (IFCREAL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 70. (IFCREAL)
    frame_width = 15. (IFCREAL)
    glass_fixing = "¢è" (IFCLABEL)
    glass_type = "¢è" (IFCLABEL)
    height = 2700. (IFCREAL)
    in_out = "O" (IFCLABEL)
    jamb_depth = 30. (IFCREAL)
    jamb_shape = "4" (IFCLABEL)
    jamb_width_side = 60. (IFCREAL)
    jamb_width_top = 60. (IFCREAL)
    manual_opener = "¢è" (IFCLABEL)
    name_of_maker = "" (IFCLABEL)
    net_shape = "¢è" (IFCLABEL)
    net_type = "¢è" (IFCLABEL)
    others = "" (IFCLABEL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "g¹ïQ" (IFCLABEL)
    sill_finish = "¢è" (IFCLABEL)
    sill_material = "¢è" (IFCLABEL)
    soundproof = "¢è" (IFCLABEL)
    type_name = "AW" (IFCLABEL)
    type_no = 23 (IFCINTEGER)
    waterproof = "¢è" (IFCLABEL)
    width = 4400. (IFCREAL)
  Pset_WindowCommon_Jpn | properties | on 1 object (1 IFCWINDOW)
    airproof = "¢è" (IFCLABEL)
    board_finish = "¢è" (IFCLABEL)
    board_material = "¢è" (IFCLABEL)
    board_thickness = 50. (IFCREAL)
    board_width = 25. (IFCREAL)
    chiri_inside = 0.01 (IFCREAL)
    chiri_outside = 0.015 (IFCREAL)
    extra_metalwork = "¢è" (IFCLABEL)
    frame_board_distance = 15. (IFCREAL)
    frame_finish = "¢è" (IFCLABEL)
    frame_material = "¢è" (IFCLABEL)
    frame_thickness = 70. (IFCREAL)
    frame_width = 15. (IFCREAL)
    glass_fixing = "¢è" (IFCLABEL)
    glass_type = "¢è" (IFCLABEL)
    height = 1200. (IFCREAL)
    in_out = "O" (IFCLABEL)
    jamb_depth = 60. (IFCREAL)
    jamb_shape = "1" (IFCLABEL)
    jamb_width_side = 60. (IFCREAL)
    jamb_width_top = 60. (IFCREAL)
    manual_opener = "¢è" (IFCLABEL)
    name_of_maker = "" (IFCLABEL)
    net_shape = "¢è" (IFCLABEL)
    net_type = "¢è" (IFCLABEL)
    others = "" (IFCLABEL)
    outside_board_width = 25. (IFCREAL)
    overhang = 85. (IFCREAL)
    product_color_number = "" (IFCLABEL)
    product_type_number = "" (IFCLABEL)
    regulation = "¢è" (IFCLABEL)
    shape = "¼J«" (IFCLABEL)
    sill_finish = "¢è" (IFCLABEL)
    sill_material = "¢è" (IFCLABEL)
    soundproof = "¢è" (IFCLABEL)
    type_name = "AW" (IFCLABEL)
    type_no = 2 (IFCINTEGER)
    waterproof = "¢è" (IFCLABEL)
    width = 1600. (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "AW-23" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "AW-1" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "AW-1" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "AW-2" (IFCLABEL)
  Pset_ColumnCommon | properties | on 12 objects (12 IFCCOLUMN)
    Reference = "500X500" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 5 objects (5 IFCCOLUMN)
    Reference = "IFC½ØÃæ" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "D500" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    Reference = "500X400" (IFCIDENTIFIER)

Other addresses and roles
  postal address (none given)